<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<text></text>
</plain>
<libraries>
<library name="Passives C-L-R">
<description>Passive Circuit Elements (C, L, &amp; R)</description>
<packages>
<package name="0805">
<description>0805</description>
</package>
<package name="4MM_SQ_L">
</package>
<package name="1210">
<description>1210</description>
</package>
<package name="1206">
<description>1206</description>
</package>
<package name="0603">
<description>0603</description>
</package>
</packages>
</library>
<library name="USB Connectors">
<description>Connector - USB Type A Plug</description>
<packages>
<package name="USB-JACK-A-TH-VER">
<description>USB-A Type Jack; TH; Vertical Insertion</description>
</package>
</packages>
</library>
<library name="MicroProcessorsSW">
<description>Microprocessors</description>
<packages>
<package name="NHD-C0216CIZ">
</package>
</packages>
</library>
<library name="Voltage Regulators - Switching">
<description>Voltage Regulator - Switching</description>
<packages>
<package name="EMSOP-8">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; Fits JEDEC packages (narrow SOIC-8)</description>
</package>
</packages>
</library>
<library name="Diodes">
<description>Diodes</description>
<packages>
<package name="SOD-123F">
</package>
<package name="SOD-323">
</package>
</packages>
</library>
<library name="Test Point">
<packages>
<package name="TP_039">
</package>
</packages>
</library>
<library name="Diodes-TVS">
<description>Diode - TVS</description>
<packages>
<package name="SMBJ-UNI">
</package>
</packages>
</library>
<library name="Pin-HeadersSW">
<description>Connector - Pin Headers</description>
<packages>
<package name="3-PIN-COM-V">
<description>Connector; 3-Pin; 1X3; 0.2" Pitch; Shroud; Vertical</description>
</package>
<package name="2-PIN-PWR">
<description>Connector; 2-Pin; 1X2; 0.2" Pitch; Shroud</description>
</package>
<package name="10-PIN-2X5-05-V-SMD">
<description>Connector; 10-Pin; 2X5; 0.05" Pitch; Vertical Mount; SMD; 3220-10-0300-00</description>
</package>
</packages>
</library>
<library name="Transistors - MOSFET">
<description>Transistors - MOSFET</description>
<packages>
<package name="SO-08">
<description>&lt;B&gt;Small Outline Narrow Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
150-mil body, package type SN</description>
</package>
<package name="SOT363">
</package>
<package name="SOT23">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
reflow soldering</description>
</package>
</packages>
</library>
<library name="Potentiometers">
<description>Potentiometers</description>
<packages>
<package name="3361P">
</package>
</packages>
</library>
<library name="Voltage Regulators - LDO">
<description>Votage Regulator - LDO</description>
<packages>
<package name="SOT89">
</package>
</packages>
</library>
<library name="Wireless Modules">
<description>Wireless Modules</description>
<packages>
<package name="SABLE_BLE">
</package>
</packages>
</library>
<library name="Frames">
<description>Frames &amp; Documentation Blocks</description>
<packages>
<package name="LETTER_L_GENERIC">
<description>Used for Standard Boards without I-CON Logo</description>
</package>
</packages>
</library>
<library name="drilegend">
<packages>
<package name="DRILEGEND">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J2" library="USB Connectors" package="USB-JACK-A-TH-VER" value="USB-JACKS-A-TH-VER">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="Passives C-L-R" package="4MM_SQ_L" value="4.7uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VR3" library="Voltage Regulators - Switching" package="EMSOP-8" value="LM2738X">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C9" library="Passives C-L-R" package="1210" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="Passives C-L-R" package="1206" value="33uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="Passives C-L-R" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CR2" library="Diodes" package="SOD-123F" value="CRS08">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CR1" library="Diodes" package="SOD-323" value="BAT54WS">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="Passives C-L-R" package="0805" value="52.5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="Passives C-L-R" package="0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="Passives C-L-R" package="0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CR3" library="Diodes" package="SOD-323" value="BAT54WS">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="Passives C-L-R" package="1206" value="33uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="+5V" library="Test Point" package="TP_039" value="TEST_POINT039">
<attribute name="NAME"/>
</element>
<element name="TVS2" library="Diodes-TVS" package="SMBJ-UNI" value="SMBJ6.8">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="12V" library="Pin-HeadersSW" package="2-PIN-PWR" value="2-PIN-HEADERS-PWR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MOTOR" library="Pin-HeadersSW" package="2-PIN-PWR" value="2-PIN-HEADERS-PWR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TEMPERATUR_SENSOR" library="Pin-HeadersSW" package="3-PIN-COM-V" value="3-PIN-HEADERS-COM-V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="MicroProcessorsSW" package="NHD-C0216CIZ" value="NHD-C0216CIZ">
<attribute name="NAME"/>
</element>
<element name="R13" library="Passives C-L-R" package="0805" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="Potentiometers" package="3361P" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="Passives C-L-R" package="0805" value="1.0K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="Passives C-L-R" package="0805" value="1.0K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="Passives C-L-R" package="0805" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="Passives C-L-R" package="0805" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="Passives C-L-R" package="0805" value=".47uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="Passives C-L-R" package="0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q5" library="Transistors - MOSFET" package="SO-08" value="MOSFET-N-P-E_H-BRIDGE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="O4" library="Test Point" package="TP_039" value="TEST_POINT039">
<attribute name="NAME"/>
</element>
<element name="O2" library="Test Point" package="TP_039" value="TEST_POINT039">
<attribute name="NAME"/>
</element>
<element name="VR1" library="Voltage Regulators - LDO" package="SOT89" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="Passives C-L-R" package="1206" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="Passives C-L-R" package="1206" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="M1" library="Wireless Modules" package="SABLE_BLE" value="SABLE_BLE"/>
<element name="Q1" library="Transistors - MOSFET" package="SOT363" value="2N7002">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="Passives C-L-R" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="Passives C-L-R" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="Transistors - MOSFET" package="SOT363" value="2N7002">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="Passives C-L-R" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="Passives C-L-R" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="Transistors - MOSFET" package="SOT363" value="2N7002">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="Passives C-L-R" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="Passives C-L-R" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q4" library="Transistors - MOSFET" package="SOT363" value="2N7002">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="Passives C-L-R" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="Passives C-L-R" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q6" library="Transistors - MOSFET" package="SOT363" value="2N7002">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="Passives C-L-R" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="Passives C-L-R" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q7" library="Transistors - MOSFET" package="SOT363" value="2N7002">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="Passives C-L-R" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="Passives C-L-R" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q8" library="Transistors - MOSFET" package="SOT363" value="2N7002">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="Passives C-L-R" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="Passives C-L-R" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q9" library="Transistors - MOSFET" package="SOT363" value="2N7002">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="Passives C-L-R" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="Passives C-L-R" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="UP" library="Pin-HeadersSW" package="2-PIN-PWR" value="2-PIN-HEADERS-PWR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="DOWN" library="Pin-HeadersSW" package="2-PIN-PWR" value="2-PIN-HEADERS-PWR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="Passives C-L-R" package="0805" value="5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="Passives C-L-R" package="0805" value="20k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="Passives C-L-R" package="0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q10" library="Transistors - MOSFET" package="SOT23" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$11" library="Frames" package="LETTER_L_GENERIC" value=""/>
<element name="P1" library="Pin-HeadersSW" package="10-PIN-2X5-05-V-SMD" value="10-PIN-HEADERS-05-V-SMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="Passives C-L-R" package="0805" value="10.0K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="Passives C-L-R" package="1206" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="Passives C-L-R" package="0805" value="10.0K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="Passives C-L-R" package="0805" value="10.0K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="Passives C-L-R" package="0805" value="10.0K"/>
<element name="DRILEGEND" library="drilegend" package="DRILEGEND" value=""/>
</elements>
<signals>
<signal name="N$1">
</signal>
<signal name="+VREG">
<contactref element="VR3" pad="2"/>
<contactref element="VR3" pad="3"/>
<contactref element="C9" pad="P1"/>
<contactref element="12V" pad="1"/>
<contactref element="CR3" pad="A"/>
<contactref element="R26" pad="2"/>
<contactref element="Q5" pad="7"/>
<contactref element="R31" pad="2"/>
</signal>
<signal name="+3V">
<contactref element="TEMPERATUR_SENSOR" pad="3"/>
<contactref element="R13" pad="2"/>
<contactref element="C2" pad="P1"/>
<contactref element="VR1" pad="3"/>
<contactref element="M1" pad="P$11"/>
<contactref element="M1" pad="P$12"/>
<contactref element="UP" pad="1"/>
<contactref element="DOWN" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="Q1" pad="5"/>
<contactref element="R7" pad="2"/>
<contactref element="Q2" pad="5"/>
<contactref element="R9" pad="2"/>
<contactref element="Q3" pad="5"/>
<contactref element="R11" pad="2"/>
<contactref element="Q4" pad="5"/>
<contactref element="R18" pad="2"/>
<contactref element="Q6" pad="5"/>
<contactref element="R20" pad="2"/>
<contactref element="Q7" pad="5"/>
<contactref element="R22" pad="2"/>
<contactref element="Q8" pad="5"/>
<contactref element="R24" pad="2"/>
<contactref element="Q9" pad="5"/>
<contactref element="R15" pad="2"/>
<contactref element="P1" pad="P$1"/>
<contactref element="C3" pad="P1"/>
</signal>
<signal name="+5V">
<contactref element="D1" pad="P$3"/>
<contactref element="R14" pad="P1"/>
<contactref element="C12" pad="P1"/>
<contactref element="L1" pad="P2"/>
<contactref element="CR1" pad="A"/>
<contactref element="C10" pad="P1"/>
<contactref element="R3" pad="2"/>
<contactref element="+5V" pad="P$1"/>
<contactref element="TVS2" pad="C"/>
<contactref element="VR1" pad="2"/>
<contactref element="C1" pad="P1"/>
<contactref element="VR1" pad="4"/>
<contactref element="R4" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="R19" pad="2"/>
<contactref element="R21" pad="2"/>
<contactref element="R23" pad="2"/>
<contactref element="Q10" pad="2"/>
</signal>
<signal name="0V">
<contactref element="J2" pad="T2"/>
<contactref element="J2" pad="4"/>
<contactref element="J2" pad="T1"/>
<contactref element="R2" pad="1"/>
<contactref element="CR2" pad="A"/>
<contactref element="C9" pad="P2"/>
<contactref element="VR3" pad="7"/>
<contactref element="VR3" pad="5"/>
<contactref element="VR3" pad="DAP"/>
<contactref element="C10" pad="P2"/>
<contactref element="C12" pad="P2"/>
<contactref element="TVS2" pad="A"/>
<contactref element="R1" pad="1"/>
<contactref element="TEMPERATUR_SENSOR" pad="1"/>
<contactref element="D1" pad="P$1"/>
<contactref element="R14" pad="P3"/>
<contactref element="12V" pad="2"/>
<contactref element="Q5" pad="3"/>
<contactref element="C1" pad="P2"/>
<contactref element="C2" pad="P2"/>
<contactref element="VR1" pad="1"/>
<contactref element="M1" pad="P$33"/>
<contactref element="M1" pad="P$34"/>
<contactref element="M1" pad="P$35"/>
<contactref element="M1" pad="P$36"/>
<contactref element="M1" pad="P$37"/>
<contactref element="M1" pad="P$38"/>
<contactref element="M1" pad="P$39"/>
<contactref element="M1" pad="P$2"/>
<contactref element="M1" pad="P$3"/>
<contactref element="M1" pad="P$22"/>
<contactref element="R30" pad="1"/>
<contactref element="P1" pad="P$3"/>
<contactref element="P1" pad="P$5"/>
<contactref element="P1" pad="P$9"/>
<contactref element="C3" pad="P2"/>
<contactref element="R16" pad="1"/>
<contactref element="R17" pad="1"/>
<contactref element="R33" pad="1"/>
</signal>
<signal name="SW">
<contactref element="L1" pad="P1"/>
<contactref element="CR2" pad="C"/>
<contactref element="VR3" pad="8"/>
<contactref element="C11" pad="2"/>
</signal>
<signal name="FB">
<contactref element="VR3" pad="6"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="BOOST">
<contactref element="VR3" pad="1"/>
<contactref element="CR1" pad="C"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="EN">
<contactref element="CR3" pad="C"/>
<contactref element="VR3" pad="4"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="TEMPERATUR_SENSOR" pad="2"/>
<contactref element="R13" pad="1"/>
<contactref element="M1" pad="P$21"/>
</signal>
<signal name="B13">
<contactref element="R9" pad="1"/>
<contactref element="Q3" pad="4"/>
<contactref element="M1" pad="P$31"/>
</signal>
<signal name="B14">
<contactref element="R11" pad="1"/>
<contactref element="Q4" pad="4"/>
<contactref element="M1" pad="P$32"/>
</signal>
<signal name="B4">
<contactref element="D1" pad="P$4"/>
<contactref element="R23" pad="1"/>
<contactref element="Q9" pad="3"/>
</signal>
<signal name="B5">
<contactref element="D1" pad="P$5"/>
<contactref element="R21" pad="1"/>
<contactref element="Q8" pad="3"/>
</signal>
<signal name="B6">
<contactref element="D1" pad="P$6"/>
<contactref element="R19" pad="1"/>
<contactref element="Q7" pad="3"/>
</signal>
<signal name="B7">
<contactref element="D1" pad="P$7"/>
<contactref element="R12" pad="1"/>
<contactref element="Q6" pad="3"/>
</signal>
<signal name="N$16">
<contactref element="R14" pad="P2"/>
<contactref element="D1" pad="P$2"/>
</signal>
<signal name="N$22">
<contactref element="R31" pad="1"/>
<contactref element="R32" pad="2"/>
<contactref element="Q5" pad="8"/>
</signal>
<signal name="N$24">
<contactref element="R29" pad="1"/>
<contactref element="C20" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="R29" pad="2"/>
<contactref element="R27" pad="1"/>
<contactref element="Q5" pad="2"/>
<contactref element="O2" pad="P$1"/>
<contactref element="MOTOR" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="C20" pad="1"/>
<contactref element="R32" pad="1"/>
<contactref element="Q5" pad="6"/>
<contactref element="O4" pad="P$1"/>
<contactref element="MOTOR" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="R26" pad="1"/>
<contactref element="R27" pad="2"/>
<contactref element="Q5" pad="5"/>
</signal>
<signal name="Z1">
<contactref element="R15" pad="1"/>
<contactref element="M1" pad="P$6"/>
<contactref element="P1" pad="P$10"/>
</signal>
<signal name="Z2">
<contactref element="M1" pad="P$7"/>
<contactref element="P1" pad="P$4"/>
</signal>
<signal name="CLOCK">
<contactref element="R4" pad="1"/>
<contactref element="Q1" pad="3"/>
<contactref element="D1" pad="P$11"/>
</signal>
<signal name="CLOCK1">
<contactref element="R6" pad="1"/>
<contactref element="Q2" pad="3"/>
<contactref element="D1" pad="P$12"/>
</signal>
<signal name="CLOCK2">
<contactref element="R8" pad="1"/>
<contactref element="Q3" pad="3"/>
<contactref element="D1" pad="P$13"/>
</signal>
<signal name="CLOCK3">
<contactref element="R10" pad="1"/>
<contactref element="Q4" pad="3"/>
<contactref element="D1" pad="P$14"/>
</signal>
<signal name="N$2">
<contactref element="R5" pad="1"/>
<contactref element="Q1" pad="4"/>
<contactref element="M1" pad="P$29"/>
</signal>
<signal name="N$3">
<contactref element="R7" pad="1"/>
<contactref element="Q2" pad="4"/>
<contactref element="M1" pad="P$30"/>
</signal>
<signal name="N1">
<contactref element="Q6" pad="4"/>
<contactref element="R18" pad="1"/>
<contactref element="M1" pad="P$15"/>
</signal>
<signal name="N2">
<contactref element="Q7" pad="4"/>
<contactref element="R20" pad="1"/>
<contactref element="M1" pad="P$16"/>
</signal>
<signal name="N3">
<contactref element="R22" pad="1"/>
<contactref element="Q8" pad="4"/>
<contactref element="M1" pad="P$17"/>
</signal>
<signal name="N4">
<contactref element="R24" pad="1"/>
<contactref element="Q9" pad="4"/>
<contactref element="M1" pad="P$18"/>
</signal>
<signal name="N$4">
<contactref element="R25" pad="2"/>
<contactref element="UP" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R25" pad="1"/>
<contactref element="R30" pad="2"/>
<contactref element="R28" pad="1"/>
<contactref element="M1" pad="P$20"/>
</signal>
<signal name="N$6">
<contactref element="R28" pad="2"/>
<contactref element="DOWN" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="Q10" pad="3"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="M1">
<contactref element="Q10" pad="1"/>
<contactref element="M1" pad="P$19"/>
<contactref element="R33" pad="2"/>
</signal>
<signal name="Z3">
<contactref element="M1" pad="P$8"/>
<contactref element="P1" pad="P$2"/>
</signal>
<signal name="Z4">
<contactref element="M1" pad="P$13"/>
<contactref element="P1" pad="P$6"/>
</signal>
<signal name="Z5">
<contactref element="M1" pad="P$14"/>
<contactref element="P1" pad="P$8"/>
</signal>
<signal name="A2">
<contactref element="M1" pad="P$23"/>
<contactref element="Q5" pad="1"/>
<contactref element="R17" pad="2"/>
</signal>
<signal name="A1">
<contactref element="M1" pad="P$24"/>
<contactref element="Q5" pad="4"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="J2" pad="2"/>
<contactref element="J2" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
