--endian=little -mv7M3 --abi=eabi -I"C:/ti/tirtos_simplelink_2_13_00_06/packages" -I"C:/ti/tirtos_simplelink_2_13_00_06/products/bios_6_42_00_08/packages" -I"C:/ti/tirtos_simplelink_2_13_00_06/products/uia_2_00_02_39/packages" -I"C:/ti/ccsv6/ccs_base" -I"C:/ti/xdctools_3_31_01_33_core/packages" -I"C:/Users/Dakota/workspace2/SimpleBLEPeripheral/FlashROM/configPkg/.." -IC:/ti/ccsv6/tools/compiler/ti-cgt-arm_5.2.6/include/rts -IC:/ti/ccsv6/tools/compiler/ti-cgt-arm_5.2.6/include  -Dxdc_target_types__="ti/targets/arm/elf/std.h" -Dxdc_target_name__=M3 -Dxdc_cfg__xheader__="\"C:/Users/Dakota/workspace2/SimpleBLEPeripheral/FlashROM/configPkg/package/cfg/appBLE_pem3.h\""
