<?xml version="1.0" encoding="UTF-8" standalone="no"?>
<configurations XML_version="1.2" id="configurations_0">
    <configuration XML_version="1.2" id="configuration_0">
        <instance XML_version="1.2" desc="Texas Instruments XDS100v3 USB Debug Probe" href="connections/TIXDS100v3_Dot7_Connection.xml" id="Texas Instruments XDS100v3 USB Debug Probe" xml="TIXDS100v3_Dot7_Connection.xml" xmlpath="connections"/>
        <connection XML_version="1.2" id="Texas Instruments XDS100v3 USB Debug Probe">
            <instance XML_version="1.2" href="drivers/tixds100v2icepick_c.xml" id="drivers" xml="tixds100v2icepick_c.xml" xmlpath="drivers"/>
            <instance XML_version="1.2" href="drivers/tixds100v2cs_dap.xml" id="drivers" xml="tixds100v2cs_dap.xml" xmlpath="drivers"/>
            <instance XML_version="1.2" href="drivers/tixds100v2cortexM.xml" id="drivers" xml="tixds100v2cortexM.xml" xmlpath="drivers"/>
            <property Type="choicelist" Value="2" id="The Converter Usage">
                <choice Name="Generate 1149.7 2-pin advanced modes" value="enable">
                    <property Type="choicelist" Value="1" id="The Converter 1149.7 Frequency">
                        <choice Name="Overclock with user specified value" value="unused">
                            <property Type="choicelist" Value="5" id="-- Choose a value from 1.0MHz to 50.0MHz"/>
                        </choice>
                    </property>
                    <property Type="choicelist" Value="5" id="The Target Scan Format"/>
                </choice>
            </property>
            <platform XML_version="1.2" id="platform_0">
                <instance XML_version="1.2" desc="CC2640F128" href="devices/cc2640f128.xml" id="CC2640F128" xml="cc2640f128.xml" xmlpath="devices"/>
            </platform>
        </connection>
    </configuration>
</configurations>
